<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.44.9-Solothurn">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>BOUNDCRS[SOURCECRS[GEOGCRS["SIRGAS-ROU98",DATUM["SIRGAS-ROU98",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],USAGE[SCOPE["Horizontal component of 3D system."],AREA["Uruguay - onshore and offshore."],BBOX[-37.77,-58.49,-30.09,-50.01]],ID["EPSG",5381]]],TARGETCRS[GEOGCRS["WGS 84",DATUM["World Geodetic System 1984",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]]],ABRIDGEDTRANSFORMATION["SIRGAS-ROU98 to WGS 84 (1)",VERSION["OGP-Ury"],METHOD["Geocentric translations (geog2D domain)",ID["EPSG",9603]],PARAMETER["X-axis translation",0,ID["EPSG",8605]],PARAMETER["Y-axis translation",0,ID["EPSG",8606]],PARAMETER["Z-axis translation",0,ID["EPSG",8607]],USAGE[SCOPE["(null/copy) Approximation for medium and low accuracy applications assuming equality between plate-fixed static and earth-fixed dynamic CRSs, ignoring static/dynamic CRS differences."],AREA["Uruguay - onshore and offshore."],BBOX[-37.77,-58.49,-30.09,-50.01]],ID["EPSG",5384],REMARK["Approximation at the +/- 1m level assuming that SIRGAS-ROU98 is equivalent to WGS 84."]]]</wkt>
      <proj4>+proj=longlat +ellps=WGS84 +towgs84=0,0,0,0,0,0,0 +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>SIRGAS-ROU98</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378137:6356752.31424517929553986</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
